**Settings for Morpho Device:**

1. Install morpho device drivers & RD services in machine.
2. Go to below path:



1. Open **ConfigSettings** file in Notepad.

Make changes as mentioned below and save the file.





Check below settings. The **RDEnviorment** Mode should be **0**

 The **CommunicationMode** should be: **0**

1. Go to windows and open ‘services.msc’.

Restart the below listed **2 services of** Morpho.

1. Go to Chrome browser and typrchrome://flags

“**Allow invalid certificates for resources loaded from localhost** “ should be **Enabled**.



1. Go to windows and open “Resource Monitor”.

The TCP Port of Morpho device should be 11100. Find below the screen shot for reference.



**Settings for Mantra Device:**

1. Install Mantra device drivers & RD services in machine for fingerprint device.
2. Go to below path :



Open Config file in Notepad.

Set the value of **env=”P”** as sown below and save the file.



1. Go to windows and open ‘services.msc’.

Restart the below listed **“Mantra ADM” service**.

If any other service of Mantra is running then please stop the same.



1. Plug the device to machine. If all setup is successful then you should get the below popup.